dialdigits
dialdigits
DIGITS

The dialdigits statement dials one or more digits.

Parameters

This statement has one parameter:

digits – digits to be dialed.

Description

This statement dials one or more digits. Unlike the dialphone statement, the digits are dialed “as-is”, with no adjustments for area code, PBX prefix, etc.

    dialdigits "555-1212"

See Also

- dialphone -- dials one or more digits, adjusting for area codes, country codes, etc..

History

Version | Status | Notes
10.0 | No Change | Carried over from Panorama 6.0.